1. High Resolution products
======================================================

#. Connect to https://scc.imaa.cnr.it

#. Log-in with your username and password

#. Click on "Station "Admin"

.. figure:: media/add_hirelpp1.jpg
   :height: 369
   :width: 1037
   :scale: 100 %
   :align: center


#. In "Product settings" tab click on the "+" at the right of "HiRELPP Products"

.. figure:: media/add_hirelpp2.jpg
   :height: 369
   :width: 1037
   :scale: 100 %
   :align: center

#. Select "Min height" and "Max height"

#. Select "Product types" and "Station"

#. Select all the channels involved in the product calculation in the "Product/channel Connection"

.. IMPORTANT::
 HiRELPP products are designed to be multi-wavelength products. So do not define different HiRELPP products for different wavelengths but put all the wavelengths (channels) in the same HiRELPP product


#. Select the configuration at which the product should be connected in "System/Product Connection"

#. On the base of the emission wavelengths of the channels included in the products, specify the emission wavelengths of the channels that have to be glued (separated by comma). If you leave this field empty the glueing will be NOT performed on any channel.

#. (Optional) If among the channels included in the product, there are cross and parallel channels, select the depolarization calibration product(s) to use for their calibration under "polarization calibration product" and the "polarization option"

#. Finally press "Save" 

.. figure:: media/add_hirelpp3.jpg
   :height: 369
   :width: 1037
   :scale: 100 %
   :align: center

This is how the HiRELPP product should look like:

.. figure:: media/add_hirelpp4.jpg
   :height: 369
   :width: 1037
   :scale: 100 %
   :align: center


